**VALCAN**

Specifications for Chorus -
**ProcellaPro**

**System overview**

ProcellaPro is a non-combustible A1 fire rated, calcium silicate-based fibre cement board using cellulose fibres for structural strength. ProcellaPro is used as a building board or sheathing board for many applications where a non-combustible solution is required.

**Features and benefits:**

* Sound dampening properties
* Insulation fixings can be screwed into the panel
* High strength
* Easy to fabricate on site
* Fast lead times
* A1 fire rating to BS EN 13501-1

**Application:**

ProcellaPro can be used for internal wall linings, tile back board and externally as a rigid sheathing board.

Panels are cut from large format sheets to suite the requirements of the build application. The Vitrafix WT fixing drills a hole into the panel and then into light weight steel frame behind, the countersunk head helps to ensure smooth board surface ready for application of any required breather membranes.

**Contacts:**

* [www.valcan.co.uk](http://www.valcan.co.uk)
* enquiries@valcan.co.uk
* T: +44 (0) 1278 428 245
* **Sheathing board**
	+ **Product reference:**
		- ProcellaPro
	+ **Thickness/weight:**
		- [12 mm] - 18.56 kg/m²
		- [10 mm] - 15.47 kg/m²
	+ **Panel size (l x w):**
		- [2500 x 1250 mm]
	+ **Fire Rating to BS EN 13501-1:** A1
	+ **Manufacturer:**
		- Valcan
		- [www.valcan.co.uk](http://www.valcan.co.uk)
		- enquiries@valcan.co.uk
		- T: +44 (0) 1278 428 245
	+ **Fixings: [**VFSDPP4.838/WT] - Vitrafix Self Drill ProcellaPro WT fixing, 4.8x38mm with Countersunk Head – Consult manufacturers details for fixing layouts